########################################################################
#
#                           MassStorage.eww
#
#
########################################################################

DESCRIPTION
===========

   This example project should be used only with IAR Embedded Workbench for ARM
  It implements a MMC/SD card drive. 
  The USB2 connect LED will indicate drive activity.

COMPATIBILITY
=============

  The MassStorage example project is compatible with Olimex LPC-2478-STK
  evaluation board. By default  the project is configured to use the J-Link 
  JTAG interface.

CONFIGURATION
=============

   After power-up the controller get clock from internal RC oscillator that
  is unstable and may fail with J-Link auto detect, therefore adaptive clocking
  should always be used. The adaptive clock can be select from menu:
  Project->Options..., section Debugger->J-Link/J-Trace  JTAG Speed - Adaptive.

  Make sure that the following jumpers are correctly configured

  Jumpers:
   EXT/JLINK  - depending of power source
   ISP_E      - unfilled
   RST_E      - unfilled
   BDS_E      - unfilled
   C/SC       - SC

GETTING STARTED
===============

  1) Start the IAR Embedded Workbench for ARM.

  2) Select File->Open->Workspace...
     Open MassStorage.eww workspace:

  3) Run the program.

  4) Use a USB cable to connect the evaluation board to your PC. The first
     time a USB device is connected to your computer, Windows will
     automatically load the proper device driver. In this case, the USB
     mass storage device driver will be loaded.

     The MassStorage application is downloaded to the flash or SDRAM memory
     on the evaluation board and executed. Also note that, during board 
     operation,the USB2 connect LED will indicate drive activity.
