########################################################################
#
#                           TouchDemo.eww
#
#
########################################################################

DESCRIPTION
===========
  This example project should be used only with IAR Embedded Workbench for ARM
 It shows basic use of I/O, timer, interrupt and LCD controllers and 
 LCD touch screen.

 The LCD hardware cursor moves as the LCD touching.
  
COMPATIBILITY
=============

   The Touch demo project is compatible with  Olimex LPC-2478-STK boar
  evaluation board. By default, the project is configured to use the
  J-Link JTAG interface.

CONFIGURATION
=============

   After power-up the controller get clock from internal RC oscillator that
  is unstable and may fail with J-Link auto detect, therefore adaptive clocking
  should always be used. The adaptive clock can be select from menu:
  Project->Options..., section Debugger->J-Link/J-Trace  JTAG Speed - Adaptive.

  Jumpers:
    EXT/JLINK  - depending of power source
    ISP_E      - unfilled
    RST_E      - unfilled
    BDS_E      - unfilled
    C/SC       - SC
  
GETTING STARTED
===============

  1) Start the IAR Embedded Workbench for ARM.

  2) Select File->Open->Workspace...
     Open TouchDemo.eww	 workspace:

  3) Run the program.

  The Touch demo application is downloaded to the iFlash or SDRAM memory.
  
