Getting Started: Running the “Device – Audio – Speaker” demo

Required Hardware: 1

Configuration 1: PICDEM FS USB + Speech Playback PICtail Plus Daughter Board. 1

Configuration 2: PIC18F87J50 PIM + HPC Explorer + Speech Playback PICtail Plus Daughter Board 1

Configuration 3: PIC18F46J50 Full Speed USB Demo Board + HPC Explorer + Speech Playback PICtail Plus Daughter Board. 1

Configuration 4: Explorer 16. 2

Configuring the Hardware: 2

Configuration 1: PICDEM FS USB + Speech Playback PICtail Plus Daughter Board. 2

Configuration 2: PIC18F87J50 PIM + HPC Explorer + Speech Playback PICtail Plus Daughter Board 3

Configuration 3: PIC18F46J50 Full Speed USB Demo Board + HPC Explorer + Speech Playback PICtail Plus Daughter Board. 4

Configuration 4: Explorer 16. 5

Firmware. 7

Audio Speaker Specification: 7

Audio Topology. 7

Running the Demo. 8

Trademarks: 8

## Required Hardware:

To run this project, you will need one of the following sets of hardware:

### Configuration 1: PICDEM FS USB + Speech Playback PICtail Plus Daughter Board

PICDEM FS USB (DM163025)

Speech Playback PICtail Plus Daughter Board (AC164125)

### Configuration 2: PIC18F87J50 PIM + HPC Explorer + Speech Playback PICtail Plus Daughter Board

PIC18F87J50 Plug-In-Module (PIM) (MA180021)

PICDEM HPC Explorer Board (DM183022)

Speech Playback PICtail Plus Daughter Board (AC164125)

### Configuration 3: PIC18F46J50 Full Speed USB Demo Board + HPC Explorer + Speech Playback PICtail Plus Daughter Board

PIC18F46J50 Full Speed USB Demo Board

PICDEM HPC Explorer Board (DM183022)

Speech Playback PICtail Plus Daughter Board (AC164125)

### Configuration 4: Explorer 16

Explorer 16 (DM240001)

USB PICtail™ Plus Daughter Card (AC164131)

Speech Playback PICtail Plus Daughter Board (AC164125)

And one of the following PIMs

PIC24FJ64GB004 Plug-In-Module (PIM) (MA240019)

PIC24FJ256GB110 Plug-In-Module (PIM) (MA240014)

PIC32MX USB Plug-In-Module (PIM) (MA320002

dsPIC33EP512MU810 Plug-In-Module (PIM)

PIC24EP512GU810 Plug-In-Module (PIM)

## Configuring the Hardware:

This section describes how to set up the various configurations of hardware to run this demo.

Configuration 1: PICDEM FS USB

Configuration 2: PIC18F87J50 PIM + HPC Explorer

Configuration 4: PIC18F46J50 Full Speed USB Demo Board + HPC Explorer

Configuration 3: Explorer 16

### Configuration 1: PICDEM FS USB + Speech Playback PICtail Plus Daughter Board

1) If using the PICDEM FS USB Demo Board, no hardware related configuration or jumper setting changes should be necessary. The Speech Playback PICtail Plus Daughter Board needs to be inserted on the PICtail™ Expansion connector on the PICDEMFS USB board.

+

Speech Playback Plus Daughter Board

PICDEMFSUSB board

### Configuration 2: PIC18F87J50 PIM + HPC Explorer + Speech Playback PICtail Plus Daughter Board

1) Before attaching the PIC18F87J50 PIM to the HPC Explorer board, insure that the processor selector switch (S3) is in the “ICE” position as seen in the image below. Failure to so will result in difficulties in getting the PIC18F87J50 PIM to sit properly on the HPC Explorer.

2) Short JP4 on the PIC18F87J50 PIM. This allows the demo board to be powered through bus power.

2) Short JP1 such that the “R” and “U” options are shorted.

3) Short JP5 on PIC18F87J50 PIM. This connects the LEDs to RE0 and RE1 pins of the Microcontroller.

4) Before connecting the PIM to HPC Explorer, remove all attached cables from both boards. Connect the PIM to the HPC Explorer board. Be careful when connecting the boards to insure that no pins are bent or damaged during the process. Also insure that the PIM is not shifted in any direction and that all of the headers are properly aligned.

### Configuration 3: PIC18F46J50 Full Speed USB Demo Board + HPC Explorer + Speech Playback PICtail Plus Daughter Board

1) Short JP3 to allow the board to be powered from the USB.

2) Short JP1 between I and R options. This connects PWM output (RC2) to the Speech Playback Card.

3) Before connecting the PIM to HPC Explorer, remove all attached cables from both boards. Connect the PIM to the HPC Explorer board. Be careful when connecting the boards to insure that no pins are bent or damaged during the process. Also insure that the PIM is not shifted in any direction and that all of the headers are properly aligned.

### Configuration 4: Explorer 16

1) Before attaching the PIM to the Explorer 16 board, insure that the processor selector switch (S2) is in the “PIM” position as seen in the image below.

2) Short the J7 jumper to the “PIC24” setting

3) Before connecting the PIM to the Explorer 16 board, remove all attached cables from both boards. Connect the PIM to the Explorer 16 board. Be careful when connecting the boards to insure that no pins are bent or damaged during the process. Also insure that the PIM is not shifted in any direction and that all of the headers are properly aligned.

3a) If using the PIC24FJ64GB004 PIM, please insure that the programming port switch is switched in the PGX1 direction.

4) On the USB PICTail Plus board, short jumper JP1. Remove all other shorts on the board.

5) Connect the USB PICTail Plus board to either of the female PICTail Plus connectors or on the card edge connector (J9) at the edge of the Explorer 16 board.

Note: When using the HID bootloader for PIC32, it is important to modify the procdefs.ld file to relocate the sections of code that will hold the bootloader and those sections that will hold the user application. Example modified procdefs.ld files have been provided with each project. This file is currently named “Procdefs.ld.boot”. When using the example project with the bootloader it is required to remove the “.boot” section of the file. This will allow MPLAB to use this file instead of the default linker file. Once the linker file is renamed, however, the project will no longer work without the bootloader. Please rename the file in order to get the project working again with PIC32.

Firmware:

To run this project, you will need to load the corresponding firmware into the devices. There are two methods available for loading the demos: Precompiled demos and source code projects.

Precompiled Demos are available in the “<Install Directory>\USB – Precompiled Demos” folders. Each demo should be prefaced with the hardware platform it is compiled for. Select the file that matches the hardware that you have and the demo that you want to run. For more information about how to load a precompiled project, please see the “Getting Started – Loading a precompiled demo” guide.

The source code for this demo is available in the “<Install Directory\USB Device – Audio – Speaker” directory. In this directory you will find all of the user level source and header files as well as project and workspace files for each of the hardware platforms. Find the project (*.mcp) or workspace (*.mcw) file that corresponds to the hardware platform you wish to test. Compile and program the demo code into the hardware platform. For more help on how to compile and program projects, please refer to the MPLAB® IDE help available through the help menu of MPLAB IDE (Help->Topics…->MPLAB IDE).

Please note that when using either the C30 or C32 demo projects you will be required to select the correct processor for the demo board.

1) Open the associated project file

2) In MPLAB Select “Configure->Select Device”

3) In the device list box in the top left corner of that window, select the desired device.

## Audio Speaker Specification:

Sampling rate of 48 KHz

1 Channel (Mono)

PCM Format - 16 bits per Sample

Asynchronous Audio Endpoint

### Audio Topology

In the demo the Feature unit implements only the Mute Control.

Running the Demo:

This demo uses the selected hardware platform as a USB Sound Playback Device.

In order to run this demo first compile and program the target device. Attach the device to the host with the USB cable. Start an audio playback at the host to run the demo.

## Trademarks:

The Microchip name and logo, the Microchip logo, MPLAB, and PIC are registered trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

PICDEM and PICTail are registered trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

Microsoft, Windows, and Windows Vista are either registered trademarks or trademarks of Microsoft Corporation in the United States and/or other countries.