| Microchip TCP/IP Stack

Home | Features | Architecture | Stack Footprint

Welcome! Stack version: Unknown Build date: Unknown This site is used to demonstrate the power and abilities of an 8 or 16-bit embedded web server. This site is powered by a Microchip PIC microcontroller running a Microchip TCP/IP Stack. Everything you see is served through a Microchip ENC28J60 10Base-T Ethernet controller or the PIC18F97J60 family Ethernet module. The bottom portion of this page illustrates real-time control of the demo board. The "Status" |  | section refreshes with board information periodically using JavaScript and the "Actions" section issues commands to toggle the on-board LEDs or LCD text (if LCD module is present). You can push the on-board switch(es) or rotate the potentiometer and see the new data. You may also click on one of the two LED command buttons to toggle on-board LEDs. If your browser does not support AJAX, you may wish to see this page for an easily refreshable static snapshot of the board state with control options.

Actions
Toggle LEDs: |  |
Write to LCD: |  |
Status

Loading...