~inc:header.inc~

# Reboot In Progress...

Your settings were successfully saved, and the board is now rebooting to configure itself with the new settings.

Your board is now located at: http://~rebootaddr~/

######

### Reconnection Instructions

1. Did you change the hostname, IP or MAC address?
   It is necessary to clear the address caches in your web browser and OS. From the command prompt in Windows, enter "nbtstat -R" to clear the hostname cache, close your current web browser, open a new web browser, and then try to access the web address above.
2. Did you try the IP address?
   Try accessing the board directly at the IP address shown on the LCD screen. (ex: enter "http://192.168.5.23/" into your browser). If this fails, then the IP address you set is not reachable. Try the step below.
3. Still not working?
   You can restore compile-time settings by clearing the board's EEPROM. Hold BTN0 (right most button on PICDEM.netTM 2 and Explorer 16) and press MCLR. Continue holding BTN0 until the LEDs flash. Release BTN0 and press MCLR again. This procedure restores the configuration settings in `TCPIPConfig.h`. You'll be able to access the board as you did when first connecting. See the Microchip TCP/IP Stack Help distributed with the stack for instructions. (If you are using an MPLAB ICD 3 or MPLAB REAL ICETM in debug mode, MCLR will not work and you'll need to reset the board via the MPLAB IDE.)

~inc:footer.inc~