/******************** (C) COPYRIGHT 2006 STMicroelectronics **********************
* File Name          : Readme.txt
* Author             : MCD Application Team
* Date First Issued  :  05/18/2006 : Version 1.0
* Description        : Description of the WDG example
**********************************************************************************
* History:
* 05/24/2006 : Version 1.1
* 05/18/2006 : Version 1.0
*********************************************************************************
 THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH
 CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
 AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT
 OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT
 OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION
 CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
**********************************************************************************

Example description
===================
This example configures the watchdog pripheral on watchdog mode in order to generate 
a system Reset each 1s.
After a Reset the system changes the state of GPIO3 port: p3.2. 
(changes the state of a led "LD3" mounted on STR912-SK-IAR board).

The wdg use the RTC 32Khz clock as clock source.

Directory contents
==================
91x_conf.h Library Configuration file
main.c      Main program
Readme.tx   This file.

How to use it
=============
In order to make the program work, you must do the following :

- Run the example


******************* (C) COPYRIGHT 2006 STMicroelectronics *****END OF FILE****
