/******************** (C) COPYRIGHT 2006 STMicroelectronics **********************
* File Name          : Readme.txt
* Author             : MCD Application Team
* Date First Issued  :  05/18/2006 : Version 1.0
* Description        : Description of the WDG example
**********************************************************************************
* History:
* 05/24/2006 : Version 1.1
* 05/18/2006 : Version 1.0
*********************************************************************************
 THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH
 CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
 AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT
 OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT
 OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION
 CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
**********************************************************************************

Example description
===================
This example configures the watchdog in timer mode and enables the generation
of an End Of count interrupt each 0.67s. For each End Of count, the system changes
the state of GPIO3 port: p3.2. (changes the state of a led "LD3" mounted on
STR912-SK-IAR board).
The wdg use the APB 25Mhz clock as clock source.

Directory contents
==================
91x_conf.h Library Configuration file
91x_it.c    Interrupt handlers
main.c      Main program
Readme.tx   This file.

How to use it
=============
In order to make the program work, you must do the following :

- Run the example


******************* (C) COPYRIGHT 2006 STMicroelectronics *****END OF FILE****
